

FOR S/W UPGRADE

1, put the MstarUpgrade.bin file in the Root of a USB device. Connect the USB device to the USB2.0 port of the TV set. Please notice that the USB3.0 port could not be used in s/w upgrading.



Root of a USB Device




Use the USB2.0 port marking in red circle

2, Normally, there are two methods to upgrade the s/w for the smart TV.

2-1, Keep the TV set in standby mode, press and hold the power key for a while(Can wait till there is upgrading OSD in the screen and the LED will keep flashing).



Power key marking in RED cycle for information.



Upgrading OSD

2-2, To select the update option in factory menu OSD.

2-2-1, Press Menu then press 1201 with the Main Menu OSD in the screen, it will go into factory OSD.




Factory menu OSD

2-2-2, Select Other Options item and then go into Other Option page, then select the Upgrade Main item. Showing as below:



Other option page

2-2-3, Select Confirm item in coming OSD after above step. The TV set will go into standby mode. Press power key (in remote or keyboard), the upgrading process will start.



Upgrade confirming

When it start upgrading, there will be upgrading OSD in the screen and the LED will keep flashing.

Note: Please do not switch off the TV set during s/w upgrading or the system will damage.